{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["清单参数明细"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"清单参数明细","index":0,"n_rows":9,"n_cols":11,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,10,1,10],[0,0,1,1],[0,2,1,9],[8,1,8,7],[5,3,5,4],[6,3,6,4],[7,3,7,4],[2,0,2,2],[2,6,2,7],[3,0,3,1],[3,6,3,7],[4,0,4,1],[4,6,4,7],[2,5,3,5]]}
[null,null,"室内P1.5小间距LED显示系统设备清单明细",{"$nulls":7},"报价单位：人民币（元）"]
[]
["预估尺寸",null,null,"屏体净显示面积(m2)",{"$f":"E4*E5","v":12.167999999999999},"独立主控数量(台)","总数(个)",null,null,"整屏点数(点)",{"$f":"K4*K5","v":5140979.9999999991}]
["长(m)",null,4.68,"长(m)",{"$f":"C4","v":4.68},null,"横向(列)",null,{"$f":"E4/0.32","v":14.624999999999998},"横向(点)",{"$f":"208*I4","v":3041.9999999999995}]
["高(m)",null,2.6,"高(m)",{"$f":"C5","v":2.6},null,"纵向(行)",null,{"$f":"E5/0.16","v":16.25},"纵向(点)",{"$f":"104*I5","v":1690}]
["序号","设备名称","型号规格","技术参数",null,"品牌"," 数量","单位","单价","总价","要求"]
[1,"室内小间距\nLED显示屏","FS-EIA1.5S","1) 输入功率 (最大值)：500 W/m²\n2) 工作温湿度：-20℃~+45℃/10%~95%RH\n3) 灰度等级：65536 levels per color",null,"大华",{"$f":"E3","v":12.167999999999999},"平方"]
[2,"大屏控制器","V1160","1、支持常见的视频接口，包括1路3G-SDI，2路HDMI1.4，1路DVI，支持3个窗口。\n2、支持10路千兆网口输出，最宽10240像素，最高8192像素带载；\n3、支持快捷配屏和高级配屏功能。\n4、支持HDMI、DVI输入分辨率自定义调节。\n5、支持设备间备份设置。\n6、支持HDMI伴随音频输入，支持3.4mm独立音频输入和输出；支持多功能卡进行音频输出；\n7、支持画质调整，亮度、对比度、饱和度和色度调整；\n8、视频输出最大带载高达650万像素。\n9、支持带载屏体亮度调节。\n10、支持一键将优先级最高的窗口全屏自动缩放。\n11、支持创建10个用户场景作为模板保存，方便使用。",null,"诺瓦",1,"台"]
[3,"合计"]